**Camden Show – Carousel**


**Assembly Instructions**

****


Printing

This model can be printed in PLA with infill of 20 percent. Support is not required except for the Top Cap. Because of tight tolerances and some printer alignments slight sanding of roof pieces and hole openings may be required.


1. Glue the Adaptor pin into the Top piece.




1. Fit the Centre section into the Top Assembly and glue the pins from the top.




1. Insert the four Horses through the top holes.




1. Fit the bottom section through the lower Horse pieces.




1. Fit the four Adaptor pins through both pieces. Glue both ends of the Horse pieces from the top and bottom. Glue the four Adaptor pins in place.




1. Fit the centre roof support onto the locating pin. Make sure that it is aligned and glue in place.




1. Fit each roof section making sure that they are located properly on the centre support.




1. Fit all eight roof pieces in place. No glue is required.



1. Fit the Top Cap and glue in place. This holds all roof pieces in place.



1. Fit and glue the “Camden Show” and “1886” plates in place on the locating pins.



**Your Carousel is now complete.**